|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Field Specimen Number | Artifact | Use Location (PC) | Activity | Notes |  |
| 16 | Flake tool | 5 and 6 | Soft material butchery | PC 5 and 6 exhibit typical bifacial butchery wear. | |
| 1326 | Flake tool with graver | 3 and 4  8, shaped spur | Soft material butchery, hide cutting | PC 3 and 4 exhibit typical bifacial butchery wear. PC 8 is a small spur with greasy, grainy polish it also has small feather and step terminations indicating it may also have been used during the butchery process. | |
| 1349 | Flake tool fragment | 2 and 3 | Possible butchery, longitudinal use | This artifact is identified as “possible” butchery due to the lack of polish and the presence of weathering along the margins of the tool which made analysis difficult. | |
| 1547 | Flake tool with graver | 7 and 8  1, graver tip | Soft material butchery, pouch polish | Arises upon the body of the artifact appear heavily weathered, this may be characteristic of “pouch polish.” Graver tip appears to have been used to puncture hides, it has a greasy appearance and if heavily rounded and smooth. | |
| 1917 & 1922 | Conjoined flake tool | 2 and 3  6 and 7 | Butchery | Both of the long edges of the tool were utilized for cutting and butchery tasks. | |
| 3013 | Flake tool fragment | N/A | Unutilized | Possible that retouching removed previous utilization traces. | |
| 3055 | Flake tool fragment | N/A | Indeterminate | Post depositional damage precluded positive identification of wear traces. | |
| 3840 & 4399 | Conjoined flake tool | 6 and 7 | Butchery | PC 6 and 7 exhibit typical bifacial butchery wear. | |
| 4624 | Scraper (burned) | 3 and 4 | Hide scraping | Heavy edge rounding in addition to more typical hide working damage. | |
| 6862 | Clovis point | 1 and 8; Central body of artifact | Projectile damage | Large impact fracture on the projectile tip, numerous small removals along margins, and striations running parallel to the working edge. | |